5       	 <--SHAPES
4       	 <--LINES
id1
2       	 <--TYPE
284       	 <--LEFT
60       	 <--TOP
70       	 <--WIDTH
30       	 <--HEIGHT
16777215       	 <--BACKCOLOR
0       	 <--BORDERCOLOR
0       	 <--BORDERCOLOR
-reserved 1-
-reserved 2-
START



id2
2       	 <--TYPE
284       	 <--LEFT
423       	 <--TOP
70       	 <--WIDTH
30       	 <--HEIGHT
16777215       	 <--BACKCOLOR
0       	 <--BORDERCOLOR
0       	 <--BORDERCOLOR
-reserved 1-
-reserved 2-
STOP



id3
91       	 <--TYPE
264       	 <--LEFT
125       	 <--TOP
111       	 <--WIDTH
40       	 <--HEIGHT
16777215       	 <--BACKCOLOR
0       	 <--BORDERCOLOR
0       	 <--BORDERCOLOR
-reserved 1-
-reserved 2-
INPUT
輸入溫度
C

id4
93       	 <--TYPE
229       	 <--LEFT
220       	 <--TOP
181       	 <--WIDTH
40       	 <--HEIGHT
16777215       	 <--BACKCOLOR
0       	 <--BORDERCOLOR
0       	 <--BORDERCOLOR
-reserved 1-
-reserved 2-
FUNCTION
溫度轉換函數
C|
F
id5
91       	 <--TYPE
228       	 <--LEFT
314       	 <--TOP
182       	 <--WIDTH
40       	 <--HEIGHT
16777215       	 <--BACKCOLOR
0       	 <--BORDERCOLOR
0       	 <--BORDERCOLOR
-reserved 1-
-reserved 2-
OUTPUT
輸出華氏溫度 = 
F

  
---- LINES ---- from,to ----
id1,id3
reserved 1

id3,id4
reserved 1

id4,id5
reserved 1

id5,id2
reserved 1

